<patchinfo incident="10">
  <!-- generated from request(s) 336929 -->
  <issue tracker="bnc" id="1084909">trackerbug: packages do not build reproducibly from hostname</issue>
  <issue tracker="bnc" id="1220065">VUL-0: CVE-2024-26328: qemu: invalid NumVFs value is mishandled in NVME SR/IOV implementation</issue>
  <issue tracker="bnc" id="1220310">Qemu cmdline core dumped with more(8193 or more) cpus</issue>
  <issue tracker="bnc" id="1222218">[HPE Bug]: virt-manager looses connection to linux guest</issue>
  <issue tracker="bnc" id="1222841">VUL-0: CVE-2024-3567: qemu: net: assertion failure in update_sctp_checksum()</issue>
  <issue tracker="bnc" id="1222843">VUL-0: CVE-2024-3446: qemu: virtio: DMA reentrancy issue leads to double free vulnerability</issue>
  <issue tracker="bnc" id="1222845">VUL-0: CVE-2024-3447: qemu: sdhci: heap buffer overflow in sdhci_write_dataport()</issue>
  <issue tracker="bnc" id="1224179">SLES 15 SP6 - KVM : Live migration of guest with multiple qcow devices remains incomplete.</issue>
  <issue tracker="cve" id="2024-3446"/>
  <issue tracker="cve" id="2024-3447"/>
  <issue tracker="cve" id="2024-3567"/>
  <issue tracker="cve" id="2024-26328"/>
  <packager>dfaggioli</packager>
  <rating>critical</rating>
  <category>security</category>
  <summary>Security update for qemu</summary>
  <description>This update for qemu fixes the following issues:

- Update to version 8.2.5:
  * target/loongarch: fix a wrong print in cpu dump
  * ui/sdl2: Allow host to power down screen
  * target/i386: fix SSE and SSE2 feature check
  * target/i386: fix xsave.flat from kvm-unit-tests
  * disas/riscv: Decode all of the pmpcfg and pmpaddr CSRs
  * target/riscv/kvm.c: Fix the hart bit setting of AIA
  * target/riscv: rvzicbo: Fixup CBO extension register calculation
  * target/riscv: do not set mtval2 for non guest-page faults
  * target/riscv: prioritize pmp errors in raise_mmu_exception()
  * target/riscv: rvv: Remove redudant SEW checking for vector fp narrow/widen instructions
  * target/riscv: rvv: Check single width operator for vfncvt.rod.f.f.w
  * target/riscv: rvv: Check single width operator for vector fp widen instructions
  * target/riscv: rvv: Fix Zvfhmin checking for vfwcvt.f.f.v and vfncvt.f.f.w instructions
  * target/riscv/cpu.c: fix Zvkb extension config
  * target/riscv: Fix the element agnostic function problem
  * target/riscv/kvm: tolerate KVM disable ext errors
  * hw/intc/riscv_aplic: APLICs should add child earlier than realize
  * iotests: test NBD+TLS+iothread
  * qio: Inherit follow_coroutine_ctx across TLS
  * target/arm: Disable SVE extensions when SVE is disabled
  * hw/intc/arm_gic: Fix handling of NS view of GICC_APR&lt;n&gt;
  * hvf: arm: Fix encodings for ID_AA64PFR1_EL1 and debug System registers
  * gitlab: use 'setarch -R' to workaround tsan bug
  * gitlab: use $MAKE instead of 'make'
  * dockerfiles: add 'MAKE' env variable to remaining containers
  * gitlab: Update msys2-64bit runner tags
  * target/i386: no single-step exception after MOV or POP SS

- Update to version 8.2.4.
  * target/sh4: Fix SUBV opcode
  * target/sh4: Fix ADDV opcode
  * hw/arm/npcm7xx: Store derivative OTP fuse key in little endian
  * hw/dmax/xlnx_dpdma: fix handling of address_extension descriptor fields
  * hw/ufs: Fix buffer overflow bug
  * tests/avocado: update sunxi kernel from armbian to 6.6.16
  * target/loongarch/cpu.c: typo fix: expection
  * backends/cryptodev-builtin: Fix local_error leaks
  * nbd/server: Mark negotiation functions as coroutine_fn
  * nbd/server: do not poll within a coroutine context
  * linux-user: do_setsockopt: fix SOL_ALG.ALG_SET_KEY
  * target/riscv/kvm: change timer regs size to u64
  * target/riscv/kvm: change KVM_REG_RISCV_FP_D to u64
  * target/riscv/kvm: change KVM_REG_RISCV_FP_F to u32

- Update to version 8.2.3.
  * Update version for 8.2.3 release
  * ppc/spapr: Initialize max_cpus limit to SPAPR_IRQ_NR_IPIS.
  * ppc/spapr: Introduce SPAPR_IRQ_NR_IPIS to refer IRQ range for CPU IPIs.
  * hw/pci-host/ppc440_pcix: Do not expose a bridge device on PCI bus
  * hw/isa/vt82c686: Keep track of PIRQ/PINT pins separately
  * virtio-pci: fix use of a released vector
  * linux-user/x86_64: Handle the vsyscall page in open_self_maps_{2,4}
  * hw/audio/virtio-snd: Remove unused assignment
  * hw/net/net_tx_pkt: Fix overrun in update_sctp_checksum()
  * hw/sd/sdhci: Do not update TRNMOD when Command Inhibit (DAT) is set
  * hw/net/lan9118: Fix overflow in MIL TX FIFO
  * hw/net/lan9118: Replace magic '2048' value by MIL_TXFIFO_SIZE definition
  * backends/cryptodev: Do not abort for invalid session ID
  * hw/misc/applesmc: Fix memory leak in reset() handler
  * hw/block/nand: Fix out-of-bound access in NAND block buffer
  * hw/block/nand: Have blk_load() take unsigned offset and return boolean
  * hw/block/nand: Factor nand_load_iolen() method out
  * qemu-options: Fix CXL Fixed Memory Window interleave-granularity typo
  * hw/virtio/virtio-crypto: Protect from DMA re-entrancy bugs
  * hw/char/virtio-serial-bus: Protect from DMA re-entrancy bugs
  * hw/display/virtio-gpu: Protect from DMA re-entrancy bugs
  * mirror: Don't call job_pause_point() under graph lock (bsc#1224179)

- Backports and bugfixes:
  * hw/net/net_tx_pkt: Fix overrun in update_sctp_checksum() (bsc#1222841, CVE-2024-3567)
  * hw/virtio/virtio-crypto: Protect from DMA re-entrancy bugs (bsc#1222843, CVE-2024-3446)
  * hw/char/virtio-serial-bus: Protect from DMA re-entrancy bugs (bsc#1222843, CVE-2024-3446)
  * hw/display/virtio-gpu: Protect from DMA re-entrancy bugs (bsc#1222843, CVE-2024-3446)
  * hw/virtio: Introduce virtio_bh_new_guarded() helper (bsc#1222843, CVE-2024-3446)
  * hw/sd/sdhci: Do not update TRNMOD when Command Inhibit (DAT) is set (bsc#1222845, CVE-2024-3447)
  * hw/nvme: Use pcie_sriov_num_vfs() (bsc#1220065, CVE-2024-26328)

- Update to version 8.2.2
  * chardev/char-socket: Fix TLS io channels sending too much data to the backend
  * tests/unit/test-util-sockets: Remove temporary file after test
  * hw/usb/bus.c: PCAP adding 0xA in Windows version
  * hw/intc/Kconfig: Fix GIC settings when using "--without-default-devices"
  * gitlab: force allow use of pip in Cirrus jobs
  * tests/vm: avoid re-building the VM images all the time
  * tests/vm: update openbsd image to 7.4
  * target/i386: leave the A20 bit set in the final NPT walk
  * target/i386: remove unnecessary/wrong application of the A20 mask
  * target/i386: Fix physical address truncation
  * target/i386: check validity of VMCB addresses
  * target/i386: mask high bits of CR3 in 32-bit mode
  * pl031: Update last RTCLR value on write in case it's read back
  * hw/nvme: fix invalid endian conversion
  * update edk2 binaries to edk2-stable202402
  * update edk2 submodule to edk2-stable202402
  * target/ppc: Fix crash on machine check caused by ifetch
  * target/ppc: Fix lxv/stxv MSR facility check
  * .gitlab-ci.d/windows.yml: Drop msys2-32bit job
  * system/vl: Update description for input grab key
  * docs/system: Update description for input grab key
  * hw/hppa/Kconfig: Fix building with "configure --without-default-devices"
  * tests/qtest: Depend on dbus_display1_dep
  * meson: Explicitly specify dbus-display1.h dependency
  * audio: Depend on dbus_display1_dep
  * ui/console: Fix console resize with placeholder surface
  * ui/clipboard: add asserts for update and request
  * ui/clipboard: mark type as not available when there is no data
  * ui: reject extended clipboard message if not activated
  * target/i386: Generate an illegal opcode exception on cmp instructions with lock prefix
  * i386/cpuid: Move leaf 7 to correct group
  * i386/cpuid: Decrease cpuid_i when skipping CPUID leaf 1F
  * i386/cpu: Mask with XCR0/XSS mask for FEAT_XSAVE_XCR0_HI and FEAT_XSAVE_XSS_HI leafs
  * i386/cpu: Clear FEAT_XSAVE_XSS_LO/HI leafs when CPUID_EXT_XSAVE is not available
  * .gitlab-ci/windows.yml: Don't install libusb or spice packages on 32-bit
  * iotests: Make 144 deterministic again
  * target/arm: Don't get MDCR_EL2 in pmu_counter_enabled() before checking ARM_FEATURE_PMU
  * target/arm: Fix SVE/SME gross MTE suppression checks
  * target/arm: Handle mte in do_ldrq, do_ldro
- Address bsc#1220310. Backported upstream commits:
  * ppc/spapr: Initialize max_cpus limit to SPAPR_IRQ_NR_IPIS
  * ppc/spapr: Introduce SPAPR_IRQ_NR_IPIS to refer IRQ range for CPU IPIs.
</description>
  <package>qemu</package>
  <package>qemu:qemu-linux-user</package>
  <seperate_build_arch/>
</patchinfo>