Based on 4c3f1641f13b7687a0dc234d3ae387b7c40494ff Mon Sep 17 00:00:00 2001
From: Lennart Poettering <lennart@poettering.net>
Date: Wed, 19 Nov 2014 20:52:23 +0100
Subject: [PATCH] core: watchdog bus properties cannot be both writable and
 constant

---
 src/core/dbus-manager.c |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- src/core/dbus-manager.c
+++ src/core/dbus-manager.c	2014-11-20 13:43:06.781518488 +0000
@@ -1599,8 +1599,8 @@ const sd_bus_vtable bus_manager_vtable[]
         SD_BUS_PROPERTY("UnitPath", "as", NULL, offsetof(Manager, lookup_paths.unit_path), SD_BUS_VTABLE_PROPERTY_CONST),
         SD_BUS_PROPERTY("DefaultStandardOutput", "s", bus_property_get_exec_output, offsetof(Manager, default_std_output), SD_BUS_VTABLE_PROPERTY_CONST),
         SD_BUS_PROPERTY("DefaultStandardError", "s", bus_property_get_exec_output, offsetof(Manager, default_std_output), SD_BUS_VTABLE_PROPERTY_CONST),
-        SD_BUS_WRITABLE_PROPERTY("RuntimeWatchdogUSec", "t", bus_property_get_usec, property_set_runtime_watchdog, offsetof(Manager, runtime_watchdog), SD_BUS_VTABLE_PROPERTY_CONST),
-        SD_BUS_WRITABLE_PROPERTY("ShutdownWatchdogUSec", "t", bus_property_get_usec, bus_property_set_usec, offsetof(Manager, shutdown_watchdog), SD_BUS_VTABLE_PROPERTY_CONST),
+        SD_BUS_WRITABLE_PROPERTY("RuntimeWatchdogUSec", "t", bus_property_get_usec, property_set_runtime_watchdog, offsetof(Manager, runtime_watchdog), 0),
+        SD_BUS_WRITABLE_PROPERTY("ShutdownWatchdogUSec", "t", bus_property_get_usec, bus_property_set_usec, offsetof(Manager, shutdown_watchdog), 0),
         SD_BUS_PROPERTY("ControlGroup", "s", NULL, offsetof(Manager, cgroup_root), 0),
 
         SD_BUS_METHOD("GetUnit", "s", "o", method_get_unit, SD_BUS_VTABLE_UNPRIVILEGED),
