From: Robert Schweikert <rjschwei@suse.com>
Date: Fri, 12 Apr 2013 12:08:16 -0400
Subject: rules: add lid switch of ARM based Chromebook as a power switch to
 logind

---
 src/login/70-power-switch.rules | 1 +
 1 file changed, 1 insertion(+)

--- a/src/login/70-power-switch.rules
+++ b/src/login/70-power-switch.rules
@@ -11,5 +11,6 @@ SUBSYSTEM=="input", KERNEL=="event*", SU
 SUBSYSTEM=="input", KERNEL=="event*", KERNELS=="thinkpad_acpi", TAG+="power-switch"
 SUBSYSTEM=="input", KERNEL=="event*", ATTRS{name}=="twl4030_pwrbutton", TAG+="power-switch"
 SUBSYSTEM=="input", KERNEL=="event*", ATTRS{name}=="tps65217_pwr_but", TAG+="power-switch"
+SUBSYSTEM=="input", KERNEL=="event*", KERNELS=="gpio-keys.8", TAG+="power-switch"
 
 LABEL="power_switch_end"
