Based on b12e56156e5f363ebb8dc4ea5c10f5fd0665dc9d Mon Sep 17 00:00:00 2001
From: David Herrmann <dh.herrmann@gmail.com>
Date: Mon, 1 Sep 2014 14:04:44 +0200
Subject: [PATCH] login: simplify controller handling

Simplify the way we handler session-controllers and fix several
shortcomings:
 * send ReleaseDevice() signals on forced session takeover
 * fix mem-leaks for busnames in case VT preparation fails (non-critical)
 * avoid passing pre-allocated names to helpers
---
 src/login/logind-session.c |   55 ++++++++++++++++++++++----------------------
 1 file changed, 28 insertions(+), 27 deletions(-)

diff --git src/login/logind-session.c src/login/logind-session.c
index 58453b5..10a43a4 100644
--- src/login/logind-session.c
+++ src/login/logind-session.c
@@ -1059,32 +1059,30 @@ bool session_is_controller(Session *s, const char *sender) {
         return streq_ptr(s->controller, sender);
 }
 
-static void session_swap_controller(Session *s, char *name) {
+static void session_release_controller(Session *s, bool notify) {
+        _cleanup_free_ char *name = NULL;
         SessionDevice *sd;
-        char *c;
 
-        if (s->controller) {
-                c = s->controller;
-                s->controller = NULL;
-                manager_drop_busname(s->manager, c);
-                free(c);
+        if (!s->controller)
+                return;
 
-                /* Drop all devices as they're now unused. Do that after the
-                 * controller is released to avoid sending out useles
-                 * dbus signals. */
-                while ((sd = hashmap_first(s->devices)))
-                        session_device_free(sd);
+        name = s->controller;
 
-                if (!name)
-                        session_restore_vt(s);
-        }
+        /* By resetting the controller before releasing the devices, we won't
+         * send notification signals. This avoids sending useless notifications
+         * if the controller is released on disconnects. */
+        if (!notify)
+                s->controller = NULL;
 
-        s->controller = name;
-        session_save(s);
+        while ((sd = hashmap_first(s->devices)))
+                session_device_free(sd);
+
+        s->controller = NULL;
+        manager_drop_busname(s->manager, name);
 }
 
 int session_set_controller(Session *s, const char *sender, bool force) {
-        char *t;
+        _cleanup_free_ char *name = NULL;
         int r;
 
         assert(s);
@@ -1095,15 +1093,13 @@ int session_set_controller(Session *s, const char *sender, bool force) {
         if (s->controller && !force)
                 return -EBUSY;
 
-        t = strdup(sender);
-        if (!t)
+        name = strdup(sender);
+        if (!name)
                 return -ENOMEM;
 
-        r = manager_watch_busname(s->manager, sender);
-        if (r) {
-                free(t);
+        r = manager_watch_busname(s->manager, name);
+        if (r)
                 return r;
-        }
 
         /* When setting a session controller, we forcibly mute the VT and set
          * it into graphics-mode. Applications can override that by changing
@@ -1115,11 +1111,14 @@ int session_set_controller(Session *s, const char *sender, bool force) {
          * or reset the VT in case it crashed/exited, too. */
         r = session_mute_vt(s);
         if (r < 0) {
-                free(t);
+                manager_drop_busname(s->manager, name);
                 return r;
         }
 
-        session_swap_controller(s, t);
+        session_release_controller(s, true);
+        s->controller = name;
+        name = NULL;
+        session_save(s);
 
         return 0;
 }
@@ -1130,7 +1129,9 @@ void session_drop_controller(Session *s) {
         if (!s->controller)
                 return;
 
-        session_swap_controller(s, NULL);
+        session_release_controller(s, false);
+        session_save(s);
+        session_restore_vt(s);
 }
 
 static const char* const session_state_table[_SESSION_STATE_MAX] = {
-- 
1.7.9.2

