From c2fa048c4a70c8386c6d8fe939e5ea9edecf1e98 Mon Sep 17 00:00:00 2001
From: David Herrmann <dh.herrmann@gmail.com>
Date: Thu, 18 Sep 2014 13:28:28 +0200
Subject: [PATCH] bus: fix bus_print_property() to use "int" for booleans

We always use "int" if we retrieve boolean values from sd-bus, as "bool"
is only a single byte, but full int on va-args.

Thanks to Werner Fink for the report!
---
 src/libsystemd/sd-bus/bus-util.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git src/libsystemd/sd-bus/bus-util.c src/libsystemd/sd-bus/bus-util.c
index 7c6da60..9018bce 100644
--- src/libsystemd/sd-bus/bus-util.c
+++ src/libsystemd/sd-bus/bus-util.c
@@ -631,7 +631,7 @@ int bus_print_property(const char *name, sd_bus_message *property, bool all) {
         }
 
         case SD_BUS_TYPE_BOOLEAN: {
-                bool b;
+                int b;
 
                 r = sd_bus_message_read_basic(property, type, &b);
                 if (r < 0)
-- 
1.7.9.2

