From 7a279c1c451cd1cf4294a9037f7acf22a6cea7d6 Mon Sep 17 00:00:00 2001
From: Alexander Graf <agraf@suse.de>
Date: Wed, 21 Feb 2018 17:41:13 +0100
Subject: [PATCH] rpi: Use firmware provided device tree

Currently the firmware generates a device tree for us that we could
just use to adjust ourselves. We then on boot throw that away and
use our own built-in device tree to configure device access.

This is bad for a multitude of reasons. For starters, it breaks
overlay support in config.txt, confusing users. Much worse however
is that we are stuck with individual U-Boot builds per board.
The firmware can easily give us the right DT depending on the
target board and revision though.

So let's use the firmware provided device tree instead. That way
U-Boot as well as payloads loaded by it can automatically adapt
to variants of RPi hardware.

Signed-off-by: Alexander Graf <agraf@suse.de>
Signed-off-by: Guillaume Gardet <guillaume.gardet@free.fr>
---
 configs/rpi_0_w_defconfig   | 2 +-
 configs/rpi_2_defconfig     | 2 +-
 configs/rpi_3_32b_defconfig | 2 +-
 configs/rpi_3_defconfig     | 2 +-
 configs/rpi_defconfig       | 2 +-
 5 files changed, 5 insertions(+), 5 deletions(-)

diff --git a/configs/rpi_0_w_defconfig b/configs/rpi_0_w_defconfig
index 39da54c3e7..81997056f4 100644
--- a/configs/rpi_0_w_defconfig
+++ b/configs/rpi_0_w_defconfig
@@ -14,7 +14,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2835-rpi-zero-w"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_2_defconfig b/configs/rpi_2_defconfig
index 5f5b40522d..06080b9347 100644
--- a/configs/rpi_2_defconfig
+++ b/configs/rpi_2_defconfig
@@ -14,7 +14,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2836-rpi-2-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_3_32b_defconfig b/configs/rpi_3_32b_defconfig
index bbf902bb91..17f672c9da 100644
--- a/configs/rpi_3_32b_defconfig
+++ b/configs/rpi_3_32b_defconfig
@@ -15,7 +15,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2837-rpi-3-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_3_defconfig b/configs/rpi_3_defconfig
index ea40351dc4..e84adb5f83 100644
--- a/configs/rpi_3_defconfig
+++ b/configs/rpi_3_defconfig
@@ -15,7 +15,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2837-rpi-3-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_defconfig b/configs/rpi_defconfig
index 981d17381a..8a2a5b83f8 100644
--- a/configs/rpi_defconfig
+++ b/configs/rpi_defconfig
@@ -14,7 +14,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2835-rpi-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
