From 2f9efa00db72a83d3591392735f67a6a559f4b14 Mon Sep 17 00:00:00 2001
From: Alexander Graf <agraf@suse.de>
Date: Mon, 2 May 2016 23:25:07 +0200
Subject: [PATCH] Revert "Revert "omap3: Use raw SPL by default for mmc1""

This reverts commit 7fa75d0ac5502db813d109c1df7bd0da34688685.
---
 arch/arm/mach-omap2/boot-common.c | 2 --
 1 file changed, 2 deletions(-)

diff --git a/arch/arm/mach-omap2/boot-common.c b/arch/arm/mach-omap2/boot-common.c
index 176d4f67cb..6fba378af9 100644
--- a/arch/arm/mach-omap2/boot-common.c
+++ b/arch/arm/mach-omap2/boot-common.c
@@ -133,8 +133,6 @@ void save_omap_boot_params(void)
 	    (boot_device <= MMC_BOOT_DEVICES_END)) {
 		switch (boot_device) {
 		case BOOT_DEVICE_MMC1:
-			boot_mode = MMCSD_MODE_FS;
-			break;
 		case BOOT_DEVICE_MMC2:
 			boot_mode = MMCSD_MODE_RAW;
 			break;
