From 7b909d7407965c03caaba30daae7aee113627a83 Mon Sep 17 00:00:00 2001
From: Josh Triplett <josh@joshtriplett.org>
Date: Tue, 11 Mar 2014 21:16:33 -0700
Subject: [PATCH] backlight: Avoid restoring brightness to an unreadably dim
 level

Some systems turn the backlight all the way off at the lowest levels.
Clamp saved brightness to at least 1 or 5% of max_brightness.  This
avoids preserving an unreadably dim screen, which would otherwise force
the user to disable state restoration.
---
 src/backlight/backlight.c |   44 ++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 44 insertions(+)

diff --git src/backlight/backlight.c src/backlight/backlight.c
index 81470b3..abf8bcf 100644
--- src/backlight/backlight.c
+++ src/backlight/backlight.c
@@ -192,6 +192,48 @@ static bool validate_device(struct udev *udev, struct udev_device *device) {
         return true;
 }
 
+/* Some systems turn the backlight all the way off at the lowest levels.
+ * clamp_brightness clamps the saved brightness to at least 1 or 5% of
+ * max_brightness.  This avoids preserving an unreadably dim screen, which
+ * would otherwise force the user to disable state restoration. */
+static void clamp_brightness(struct udev_device *device, char **value) {
+        int r;
+        const char *max_brightness_str;
+        unsigned brightness, max_brightness, new_brightness;
+
+        max_brightness_str = udev_device_get_sysattr_value(device, "max_brightness");
+        if (!max_brightness_str) {
+                log_warning("Failed to read max_brightness attribute; not checking saved brightness");
+                return;
+        }
+
+        r = safe_atou(*value, &brightness);
+        if (r < 0) {
+                log_warning("Failed to parse brightness \"%s\": %s", *value, strerror(-r));
+                return;
+        }
+
+        r = safe_atou(max_brightness_str, &max_brightness);
+        if (r < 0) {
+                log_warning("Failed to parse max_brightness \"%s\": %s", max_brightness_str, strerror(-r));
+                return;
+        }
+
+        new_brightness = MAX3(brightness, 1U, max_brightness/20);
+        if (new_brightness != brightness) {
+                char *old_value = *value;
+
+                r = asprintf(value, "%u", new_brightness);
+                if (r < 0) {
+                        log_oom();
+                        return;
+                }
+
+                log_debug("Saved brightness %s too low; increasing to %s.", old_value, *value);
+                free(old_value);
+        }
+}
+
 int main(int argc, char *argv[]) {
         _cleanup_udev_unref_ struct udev *udev = NULL;
         _cleanup_udev_device_unref_ struct udev_device *device = NULL;
@@ -306,6 +348,8 @@ int main(int argc, char *argv[]) {
                         return EXIT_FAILURE;
                 }
 
+                clamp_brightness(device, &value);
+
                 r = udev_device_set_sysattr_value(device, "brightness", value);
                 if (r < 0) {
                         log_error("Failed to write system attribute: %s", strerror(-r));
-- 
1.7.9.2

