From: Robert Milasan <rmilasan@suse.com>
Date: Wed, 27 Jun 2012 08:55:59 +0000
Subject: rules create by id scsi links for ATA devices

Re-enable creation of by-id scsi links for ATA devices. (bnc#769002)
---
 rules/60-persistent-storage.rules | 4 ++++
 1 file changed, 4 insertions(+)

--- systemd-206.orig/rules/60-persistent-storage.rules
+++ systemd-206/rules/60-persistent-storage.rules
@@ -42,6 +42,10 @@ KERNEL=="cciss*", ENV{DEVTYPE}=="disk",
 KERNEL=="sd*|sr*|cciss*", ENV{DEVTYPE}=="disk", ENV{ID_SERIAL}=="?*", SYMLINK+="disk/by-id/$env{ID_BUS}-$env{ID_SERIAL}"
 KERNEL=="sd*|cciss*", ENV{DEVTYPE}=="partition", ENV{ID_SERIAL}=="?*", SYMLINK+="disk/by-id/$env{ID_BUS}-$env{ID_SERIAL}-part%n"
 
+# scsi compat links for ATA devices
+KERNEL=="sd*[!0-9]", ENV{ID_BUS}=="ata", PROGRAM="scsi_id --whitelisted --replace-whitespace -p0x80 -d $devnode", RESULT=="?*", ENV{ID_SCSI_COMPAT}="$result", SYMLINK+="disk/by-id/scsi-$env{ID_SCSI_COMPAT}"
+KERNEL=="sd*[0-9]", ENV{ID_SCSI_COMPAT}=="?*", SYMLINK+="disk/by-id/scsi-$env{ID_SCSI_COMPAT}-part%n"
+
 # firewire
 KERNEL=="sd*[!0-9]|sr*", ATTRS{ieee1394_id}=="?*", SYMLINK+="disk/by-id/ieee1394-$attr{ieee1394_id}"
 KERNEL=="sd*[0-9]", ATTRS{ieee1394_id}=="?*", SYMLINK+="disk/by-id/ieee1394-$attr{ieee1394_id}-part%n"
