Based on 52fb538361053f8c4abce0e40cd0bae3d28ceb16 Mon Sep 17 00:00:00 2001
From: Tom Hirst <tom.hirst@ipe-systems.co.uk>
Date: Wed, 25 Jun 2014 11:57:11 +0000
Subject: [PATCH] rules: don't enable usb pm for Avocent devices

The Avocent KVM over IP devices doesn't work correctly with USB power
management enabled.
---
 rules/42-usb-hid-pm.rules |    4 ----
 1 file changed, 4 deletions(-)

diff --git rules/42-usb-hid-pm.rules rules/42-usb-hid-pm.rules
index c675b5b..4c300da 100644
--- rules/42-usb-hid-pm.rules
+++ rules/42-usb-hid-pm.rules
@@ -12,10 +12,6 @@ ACTION=="add", SUBSYSTEM=="usb", ATTR{product}=="QEMU USB Mouse", ATTR{serial}!=
 ACTION=="add", SUBSYSTEM=="usb", ATTR{product}=="QEMU USB Tablet", ATTR{serial}!="1", TEST=="power/control", ATTR{power/control}="auto"
 ACTION=="add", SUBSYSTEM=="usb", ATTR{product}=="QEMU USB Keyboard", ATTR{serial}!="1", TEST=="power/control", ATTR{power/control}="auto"
 
-# Catch-all for Avocent HID devices. Keyed off interface in order to only
-# trigger on HID class devices.
-ACTION=="add", SUBSYSTEM=="usb", ATTRS{idVendor}=="0624", ATTR{bInterfaceClass}=="03", TEST=="../power/control", ATTR{../power/control}="auto"
-
 # Dell DRAC 4
 ACTION=="add", SUBSYSTEM=="usb", ATTR{idVendor}=="413c", ATTR{idProduct}=="2500", TEST=="power/control", ATTR{power/control}="auto"
 
-- 
1.7.9.2

