From f9e1ee09fadbd4fb146d4f7bb45a6212773dff63 Mon Sep 17 00:00:00 2001
From: Hannes Reinecke <hare@suse.de>
Date: Thu, 10 Apr 2014 11:14:20 +0200
Subject: [PATCH 2/2] Skip persistent device link creation on multipath device
 paths

When a device is marked as a multipath device path by setting
DM_MULTIPATH_DEVICE_PATH="1" udev should not create any
persistent symlinks to that device.
Otherwise systemd will get confused about which device to use.

---
 rules/60-persistent-storage.rules | 7 +++++--
 1 file changed, 5 insertions(+), 2 deletions(-)

diff --git a/rules/60-persistent-storage.rules b/rules/60-persistent-storage.rules
index 1208bd3..fd5bedd 100644
--- a/rules/60-persistent-storage.rules
+++ b/rules/60-persistent-storage.rules
@@ -39,8 +39,8 @@ KERNEL=="sd*[!0-9]|sr*", ENV{ID_SERIAL}!="?*", SUBSYSTEMS=="usb", IMPORT{builtin
 # scsi devices
 KERNEL=="sd*[!0-9]|sr*", ENV{ID_SERIAL}!="?*", IMPORT{program}="scsi_id --export --whitelisted -d $devnode", ENV{ID_BUS}="scsi"
 KERNEL=="cciss*", ENV{DEVTYPE}=="disk", ENV{ID_SERIAL}!="?*", IMPORT{program}="scsi_id --export --whitelisted -d $devnode", ENV{ID_BUS}="cciss"
-KERNEL=="sd*|sr*|cciss*", ENV{DEVTYPE}=="disk", ENV{ID_SERIAL}=="?*", SYMLINK+="disk/by-id/$env{ID_BUS}-$env{ID_SERIAL}"
-KERNEL=="sd*|cciss*", ENV{DEVTYPE}=="partition", ENV{ID_SERIAL}=="?*", SYMLINK+="disk/by-id/$env{ID_BUS}-$env{ID_SERIAL}-part%n"
+KERNEL=="sd*|sr*|cciss*", ENV{DEVTYPE}=="disk", ENV{DM_MULTIPATH_DEVICE_PATH}!="1", ENV{ID_SERIAL}=="?*", SYMLINK+="disk/by-id/$env{ID_BUS}-$env{ID_SERIAL}"
+KERNEL=="sd*|cciss*", ENV{DEVTYPE}=="partition", ENV{DM_MULTIPATH_DEVICE_PATH}!="1", ENV{ID_SERIAL}=="?*", SYMLINK+="disk/by-id/$env{ID_BUS}-$env{ID_SERIAL}-part%n"
 
 # scsi compat links for ATA devices
 KERNEL=="sd*[!0-9]", ENV{ID_BUS}=="ata", PROGRAM="scsi_id --whitelisted --replace-whitespace -p0x80 -d $devnode", RESULT=="?*", ENV{ID_SCSI_COMPAT}="$result", SYMLINK+="disk/by-id/scsi-$env{ID_SCSI_COMPAT}"
@@ -70,6 +70,9 @@ KERNEL=="sr*", ENV{DISK_EJECT_REQUEST}!="?*", ENV{ID_CDROM_MEDIA_TRACK_COUNT_DAT
 KERNEL=="sr*", ENV{DISK_EJECT_REQUEST}!="?*", ENV{ID_CDROM_MEDIA_TRACK_COUNT_DATA}=="?*", ENV{ID_CDROM_MEDIA_SESSION_LAST_OFFSET}=="", \
   IMPORT{builtin}="blkid --noraid"
 
+# Skip blkid on multipath device paths
+ENV{DM_MULTIPATH_DEVICE_PATH}=="1", GOTO="persistent_storage_end"
+
 # probe filesystem metadata of disks
 KERNEL!="sr*", IMPORT{builtin}="blkid"
 
-- 
1.8.1.4

