From e75d103c47d687ecc49cb522833084ebf5da04fd Mon Sep 17 00:00:00 2001
From: Alexander Graf <agraf@suse.de>
Date: Thu, 15 Mar 2018 09:54:10 +0100
Subject: [PATCH] rpi3: Enable lan78xx driver

The new Raspberry Pi B 3+ has a lan78xx device attached to it. Let's add
driver support in U-Boot for it.

Signed-off-by: Alexander Graf <agraf@suse.de>
---
 configs/rpi_3_defconfig | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/configs/rpi_3_defconfig b/configs/rpi_3_defconfig
index ca55f8dc66..1ee04c68f8 100644
--- a/configs/rpi_3_defconfig
+++ b/configs/rpi_3_defconfig
@@ -36,3 +36,5 @@ CONFIG_SYS_WHITE_ON_BLACK=y
 CONFIG_CONSOLE_SCROLL_LINES=10
 CONFIG_PHYS_TO_BUS=y
 CONFIG_OF_LIBFDT_OVERLAY=y
+CONFIG_PHYLIB=y
+CONFIG_USB_ETHER_LAN78XX=y
